Observation attack – data should be encrypted.

Fault attack – exploit physical flaws in the card using physics. Protect using redundancy and checks.